****

**SESSION 2022**

|  |
| --- |
| **BACCALAURÉAT PROFESSIONNEL** **ÉPREUVE ORALE SPÉCIFIQUE « SECTION EUROPÉENNE »****SPÉCIALITÉ : ÉTUDE et RÉALISATION d’AGENCEMENT****LANGUE : ANGLAIS** |

**SUJET N°1**

**Durée de l’épreuve : 40 minutes**

|  |  |
| --- | --- |
| * Préparation
 | * 20 minutes
 |
| * Présentation de la situation
 | * 10 minutes
 |
| * Entretien sur les activités et travaux effectués dans la discipline non linguistique
 | * 10 minutes
 |

**SITUATION :**

You work as a technician at LDN furniture Company and you are in charge of welcoming a new temporary woodworker in your company.

The person comes to reinforce the team to produce a dressing room.

Explain to him the safety rules in the wood workshop business and the project of the dressing room he has to work on : how the room will be organized, the materials used, the joining system and more...



**DOCUMENTS :**

* **N° 1 : SAFETY RULES IN THE WORKSHOP**
* **N° 2 : PLANS OF THE DRESSING ROOM**

**DOCUMENT 1 : SAFETY RULES IN THE WORKSHOP**

## What safety procedures should you follow when using woodworking machines?

* Always wear safety glasses or goggles, or a face shield (with safety glasses or goggles).
* Wear hearing protection that is suitable for the level and frequency of the noise you are exposed to in the woodworking area.
* Use gloves to protect hands from splinters when handling wood but do not wear them near rotating blades and other machinery parts where the gloves can catch.
* Wear protective footwear.
* Make sure the guard is in position, is in good working condition, and guards the machine adequately before operating any equipment or machine. Check and adjust all other safety devices.
* Make sure the equipment is properly grounded before use.
* Check that keys and adjusting wrenches are removed from the machine before turning on the power.
* Inspect stock for nails or other materials before cutting, planning, routing or carrying out similar activities.
* Make sure that all machines have start and stop buttons.
* Turn the power off and unplug the power cord (or lock out the power source) before inspecting, changing, cleaning, adjusting or repairing a blade or a machine. Also turn the power off when discussing the work.





<http://ccohs.ca/oshanswers/safety_haz/woodwork/gen_safe.html>

**DOCUMENT 2 : PLANS OF THE DRESSING ROOM**

<https://lamco-design.co.uk/case-studies/lamco-dressing-room/>

